sb16fix - Installation Guide

1.		Login as root
2.		Install the Driver
                  
                  Important.
		This Version (1.0b) only support a SB16 and (ASP) at
		the port address 0x220 !!!!

3.               type     dread -l  |  grep NeXT1

                  You may get following  output ....

                     	NeXT1 SpeakerBalance -0.008
			NeXT1 VisualBeep No
			NeXT1 InitialKeyRepeat 15
			NeXT1 MouseScaling "5 1 1 6 2 7 3 8 5 9 7"
			NeXT1 SpeakerVolume 1.000
			NeXT1 TimeZone 11
			NeXT1 KeyRepeat 2
			NeXT1 MicrophoneBalance 0.025
			NeXT1 MicrophoneGain 1.000

                   type
			dremove NeXT1 MicrophoneBalance 0.025
			dremove NeXT1 MicrophoneGain 1.000

4. 		Repeat step 3 for each user  
		(simply by using su - username)

5.  		Reboot 

To make a  2 Channel  16bit  22100 khz recording type

                           sndrecord  -F3 -S22100 -n2 -v   test.snd	
If you have any questions or problems write an eMail to

                           schaefer@nimbus.ruhr.de 

THIS DRIVER IS PUBLIC DOMAIN AND FOR FREE USE.