Instructions for building an Intel bootable floppy set:

1. Format two disks high density disks with NeXT format.

2. Insert disk 1

3. In a terminal window, su to root and type:

	ren:1# dd if=BootDisk1.dd of=/dev/rfd0b conv=sync
	2880+0 records in
	2880+0 records out
	
4. Eject disk 1, insert disk 2

5. Type:
	
	ren:2# dd if=FsckDisk2.dd of=/dev/rfd0b conv=sync
	2880+0 records in
	2880+0 records out

To boot from these floppies, insert disk 1 and boot the machine.  When it prompts you to "Insert the filesystem", insert disk 2 and hit a key.  You will come up in single user mode and be able to fsck your hard drive.