MusicKit Synthpatches

20-October, 1992

NeXT SynthPatches:
   Wave1i   	Wavetable synthesis with 1 oscillator.
   Wave1vi   	Wavetable synthesis with 1 osc. and random and sinusoidal vibrato.
   DBWave1vi  	Same as Wave1vi, but with access to the Timbre Database.
   DBWave2vi  	Two database WaveTables with vibrato and interpolation and cross-fade.
   Fm1i   	Simple fm synthesis.
   Fm1vi   	Simple fm synthesis with vibrato.
   DBFm1vi    	Simple fm that has access to the Music Kit WaveTable database for use in the carrier.
   Fm2pvi    	Fm synthesis with 2 modulators in parallel, vibrato.
   Fm2pnvi    	Like Fm2vi, but with an additional noise modulator.
   Fm2cvi   	Fm synthesis with 2 modulators in cascade, vibrato.
   Fm2cnvi    	Like Fm2cvi, but with an additional noise modulator.
   Pluck    	Plucked string physical model.

CCRMA SynthPatches (not in current release):
   HoseIns    	Garden hose with mouthpiece physical model (bugle-like).
   ClariNot    	Clarinet physical model.
   SlideFlute   	Flute physical model.
   WhirlWind   	General instrument including the 3 above.
   RocknRole   	Plucked string with feedback physical model.
   Dumbow    	Bowed string physical model.

Synthpatches Parameters

Standard Parameters - Recognized by all SynthPatches.
	freq keyNum pitchBend pitchBendSensitivity bearing
	amp velocity velocitySensitivity controlChange controlVal
Standard Oscillator Parameters - Recognized by all but physical model SynthPatches.
	ampEnv amp0 amp1 ampAtt ampRel freqEnv freq0 freq1
	freqAtt freqRel portamento waveform waveLen phase
DBWave2vi  Parameters - Recognized for waveform cross-fade.
	 waveform0 waveform1 waveformAtt waveformRel waveformEnv
Vibrato Parameters - Recognized by SynthPatches with vibrato.
	sVibFreq sVibAmp sVibFreq0 sVibFreq1 
	sVibAmp0 sVibAmp1 rVibAmp
FM Parameters - Recognized by all FM SynthPatches.
	cRatio m1Ratio m1Ind m1IndEnv m1Ind0 m1Ind1
	m1IndAtt m1IndRel m1Waveform m1Phase bright afterTouch afterTouchSensitivity
Double FM Parameters - Recognized by bi-modulator FM SynthPatches.
	 m2Ratio m2Ind m2IndEnv m2Ind0 m2Ind1 m2IndAtt
	m2IndRel m2Waveform m2Phase
Noise Modulation Parameters - Recognized by FM noise SynthPatches.
	noiseAmp noiseAmpEnv noiseAmp0 noiseAmp1
	noiseAmpAtt noiseAmpRel breathSensitivity
MIDI Panning Parameters -Recognized by SynthPatches that support MIDI panning.
	panSensitivity
Pluck Parameters -Recognized by Pluck.
	lowestFreq sustain pickNoise decay bright velocity amp ampRel 

	(being determined) 
HoseIns Parameters -Recognized by HoseIns.
ClariNot Parameters -Recognized by ClariNot.
SlideFlute Parameters -Recognized by SlideFlute.
RocknRole Parameters -Recognized by RocknRole.
Dumbow Parameters -Recognized by Dumbow.